ISU Top Ten Safety Violations 2015

1. No chemical/bio/rad inventory
2. Incorrect container label (usually this is that they are not labeling with full chemical names)
3. Eyewash & safety shower (not tested or inaccessible )
4. No training records available or training not completed
5. No emergency action plan (or plan has outdated contact information)
6. Electrical safety issues (primarily improper use of extension cords and/or power strips)
7. Satellite accumulation area issues (top 3 SAA problems are: 1. Waste not labeled 2. No cap on the container 3. Over 90 days)
8. Signage issues
9. Safety surveys not completed by lab staff
10. PPE not available, not used or used incorrectly